12 KEY CONFIGURATIONS FOR SINGLE ZONE Cone Fire & Ramp Hold

1. HOLD THE NUMBER 4 BUTTON DOWN WHILE TURNING ON THE POWER
2. THE DISPLAY WILL READ CFG
3. ENTER THE NUMBERS (PRESS NUMBERS) 456987
4. THE DISPLAY WILL READ FLASHING BETWEEN – CFG AND 0021 OR 0005
5. PRESS 21 (CONE FIRE) – THEN PRESS ENTER
6. DISPLAY WILL THEN READ IDLE
7. USE THE OPTION BUTTON (NUMBER 0) TO SCROLL THROUGH OPTIONS
8. PRESS OPTIONS BUTTON UNTIL YOU GET TO THE ABBREVIATION TC
9. PRESS ENTER
10. USING THE #1 OR #2 BUTTON PRESS EITHER ONE UNTIL YOU SEE (K OR S) SELECT THE TYPE YOU WANT TO SELECT – (WHAT THE DISPLAY SHOULD READ)
11. PRESS ENTER
12. PRESS OPTIONS BUTTON AGAIN UNTIL YOU SEE SFTY (SAFETY)
13. PRESS ENTER
14. ENTER THE NUMBERS FOR THE MAX TEMPERATURE. (FROM WIRING DIAGRAM OR SERIAL PLATE)
15. PRESS ENTER
16. PRESS OPTIONS BUTTON AGAIN UNTIL THE DISPLAY READS CFG
17. PRESS ENTER
18. TURN OFF POWER THEN TURN POWER ON

 19. CHECK OPTIONS MAKE SURE THEY ARE CORRECT.